|  |
| --- |
|  |
| Portable Earthing Set for mains/substation (1) |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Equipment Unique Identification Number |  | Copper/Aluminium Cable (2) |

Note (1): Select ‘mains’ or ‘substation’ as required. Insert name of substation at the right box for SS use.

Note (2): Select ‘Copper’ or ‘Aluminium’ as required. If Aluminium cable, re-termination must be performed every 6 years and recorded under the ‘Comments’ column below.

The six-monthly and three-yearly inspections are to be undertaken respectively in accordance with Sections 4.3 and 4.4 of *SP D 79043 Inspection and Care of Portable Earthing Equipment for the High Voltage System*.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Inspection Interval | Date of inspection | Inspected by (Name) and/or (Company) | Result (Tick as appropriate) | | Comments (e.g. reason for fail) |
| Pass | Fail |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 3-yearly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 3-yearly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 3-yearly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 3-yearly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 6-monthly |  |  |  |  |  |
| 3-yearly |  |  |  |  |  |