|  |
| --- |
|  |
| Rail-connecting set for mains/substation (1) |

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Equipment Unique Identification Number |  |  |

Note (1): Delete ‘mains’ or ‘substation’ as required. Insert name of substation at the right box for SS use.

The six-monthly and three-yearly inspections are to be undertaken respectively in accordance with Sections 4.3 and 4.4 of *SP D 79045 Inspection and Care of Portable Rail Connecting Equipment for 1500 Volt Overhead Wiring*.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inspection Interval | Date of Inspection | Inspected by (Name) | Result(Tick as appropriate) | Comments (e.g. reason for fail) |
|  |  |  | Pass  | Fail  |  |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 3-yearly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 3-yearly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 3-yearly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 3-yearly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 6-monthly |  |  |[ ] [ ]   |
| 3-yearly |  |  |[ ] [ ]   |